**[hardware](C:/Users/86156/AppData/Local/youdao/dict/Application/8.5.2.0/resultui/html/index.html" \l "/javascript:;)** **[configuration](C:/Users/86156/AppData/Local/youdao/dict/Application/8.5.2.0/resultui/html/index.html" \l "/javascript:;)**

1. Scan configuration code，Configure for virtual serial port mode



1. Scan configuration code，Clear prefix/suffix



1. Scan configuration code，Configure custom prefix/suffixes



**[software](C:/Users/86156/AppData/Local/youdao/dict/Application/8.5.2.0/resultui/html/index.html" \l "/javascript:;)** **[configuration](C:/Users/86156/AppData/Local/youdao/dict/Application/8.5.2.0/resultui/html/index.html" \l "/javascript:;)**

1. Install the virtual serial driver, Choose the right version for you




1. Double click Opsosetup.exe, install by default, do not change the installation path




3、Find oposconfig on the desktop and double-click to open it



Connect the scanning device,Customize a scan device name.Click on “Add Device”




The following figure shows successful installation



# Sample Test

Open the folder OposDriverTest,Run DualTest.exe



Chose your device